;
; TSeng Display INF
;
[version]
signature="$CHICAGO$"
Class=Display
ClassGUID={4d36e968-e325-11ce-bfc1-08002be10318}
Provider=%MS%
SetupClass=BASE

[DestinationDirs]
DefaultDestDir  =11             ;LDID_SYS
Driver.Copy     =11

; Manufacturers
; ---------------------------------------------------------
[Manufacturer]
%Diamond%=Mfg.Diamond
%DFI%    =Mfg.DFI
%Genoa%  =Mfg.Genoa
%Herc%   =Mfg.Herc
%Orchid% =Mfg.Orchid
%STB%    =Mfg.STB
%Tseng%  =Mfg.Tseng


; Driver Sections
; ---------------------------------------------------------

[Mfg.Diamond]
%Stealth32%=TsengW32,, *PNP0912
%SpeedStar%=ET4000,, *PNP0906
%SpeedStar24%=ET4000,, *PNP0906

[Mfg.DFI]
%WG5000%=TsengW32,, *PNP0912

[Mfg.Genoa]
%Phantom32%=TsengW32,, *PNP0912

[Mfg.Herc]
%Dynamite%=TsengW32,, *PNP0912
%DynamitePro%=TsengW32,, *PNP0912

[Mfg.Orchid]
%ProDesII%=ET4000,, *PNP0906

[Mfg.STB]
%ErgoMCX%=TsengW32,, *PNP0912
%Lightspeed%=TsengW32,, *PNP0912
%MVP-2X%=TsengW32,, *PNP0912
%MVP-4X%=TsengW32,, *PNP0912

[Mfg.Tseng]
%*PNP0906.DeviceDesc%=ET4000, *PNP0906, *PNP0912, *PNP091A
%*PNP0912.DeviceDesc%=TsengW32, *PNP0912
%PCI\VEN_100C&DEV_3202.DeviceDesc%=TSENGW32, PCI\VEN_100C&DEV_3202
%PCI\VEN_100C&DEV_3205.DeviceDesc%=TSENGW32, PCI\VEN_100C&DEV_3205
%PCI\VEN_100C&DEV_3206.DeviceDesc%=TSENGW32, PCI\VEN_100C&DEV_3206
%PCI\VEN_100C&DEV_3207.DeviceDesc%=TSENGW32, PCI\VEN_100C&DEV_3207
%PCI\VEN_100C&DEV_3208.DeviceDesc%=ET6000, PCI\VEN_100C&DEV_3208



; Install Sections
; ---------------------------------------------------------

; -------------- Obsolete utility removal sections

[Diamond.IniFields]
win.ini, windows, load, *dcshkey.exe,,1

; -------------- Common sections

[Prev.DelReg]
HKR,,Ver
HKR,,DevLoader
HKR,,EnumPropPages
HKR,INFO
HKR,DEFAULT
HKR,MODES
HKR,CURRENT

[VGA.LogConfig]
ConfigPriority=HARDWIRED
IOConfig=3B0-3BB
IOConfig=3C0-3DF
MemConfig=A0000-AFFFF
MemConfig=B8000-BFFFF
MemConfig=C0000-C7FFF,D0000-D7FFF,E0000-E5FFF,E0000-E7FFF


; -------------- Tseng ET4000
[ET4000]
CopyFiles=ET4000.Copy
DelReg=Prev.DelReg
AddReg=ET4000.AddReg
LogConfig=VGA.LogConfig

[ET4000.Copy]
framebuf.drv,,,12
tseng.vxd,,,12
supervga.drv,,,12
framebuf.dll,,,12

[ET4000.AddReg]
HKR,,Ver,,4.0
HKR,,DevLoader,,*vdd
HKR,DEFAULT,Mode,,"4,640,480"
HKR,DEFAULT,drv,,framebuf.drv
HKR,DEFAULT,vdd,,"*vdd,*vflatd"
HKR,DEFAULT,minivdd,,tseng.vxd
HKR,"MODES\4\640,480",drv,,vga.drv
HKR,"MODES\4\640,480",vdd,,*vdd
HKR,"MODES\4\800,600",drv,,supervga.drv
HKR,"MODES\4\800,600",vdd,,*vdd
HKR,"MODES\8\640,480"
HKR,"MODES\8\800,600"
HKR,"MODES\8\1024,768"
HKR,"MODES\16\640,480"
HKR,"MODES\16\800,600"
HKR,"MODES\24\640,480"

; -------------- Tseng W32/W32i/W32p
[TsengW32]
CopyFiles=TsengW32.Copy
DelReg=Prev.DelReg
AddReg=TsengW32.AddReg
UpdateIniFields=Diamond.IniFields
LogConfig=VGA.LogConfig

[TsengW32.Copy]
tseng.drv,,,12
tseng.vxd,,,12
supervga.drv,,,12
tseng.dll,,,12

[TsengW32.AddReg]
HKR,,Ver,,4.0
HKR,,DevLoader,,*vdd
HKR,DEFAULT,Mode,,"8,640,480"
HKR,DEFAULT,drv,,tseng.drv
HKR,DEFAULT,vdd,,"*vdd,*vflatd"
HKR,DEFAULT,minivdd,,tseng.vxd
HKR,"MODES\4\640,480",drv,,vga.drv
HKR,"MODES\4\640,480",vdd,,*vdd
HKR,"MODES\4\800,600",drv,,supervga.drv
HKR,"MODES\4\800,600",vdd,,*vdd
HKR,"MODES\8\640,480"
HKR,"MODES\8\800,600"
HKR,"MODES\8\1024,768"
HKR,"MODES\8\1280,1024"
HKR,"MODES\16\640,480"
HKR,"MODES\16\800,600"
HKR,"MODES\16\1024,768"
HKR,"MODES\24\640,480"
HKR,"MODES\24\800,600"

[TsengW32.PosDup]

; -------------- Tseng ET6000
[ET6000]
CopyFiles=ET6000.Copy
DelReg=Prev.DelReg
AddReg=ET6000.AddReg

[ET6000.Copy]
et6000.drv,,,12
et6000.vxd,,,12
et6000.dll,,,12

[ET6000.AddReg]
HKR,,Ver,,4.0
HKR,,DevLoader,,*vdd
HKR,DEFAULT,Mode,,"8,640,480"
HKR,DEFAULT,drv,,ET6000.drv
HKR,DEFAULT,drv2,,ET6000.drv
HKR,DEFAULT,vdd,,"*vdd,*vflatd"
HKR,DEFAULT,minivdd,,ET6000.vxd
HKR,DEFAULT,RefreshRate,,0     ; DDC support
HKR,DEFAULT,DDC,,1              ; DDC support
HKR,"MODES\4\640,480",drv,,vga.drv
HKR,"MODES\4\640,480",vdd,,*vdd
HKR,"MODES\4\800,600",drv,,supervga.drv
HKR,"MODES\4\800,600",vdd,,*vdd
HKR,"MODES\8\640,480",,,"60,72,75,90"
HKR,"MODES\8\800,600",,,"60,72,75,90"
HKR,"MODES\8\1024,768",,,"60,70,75"
HKR,"MODES\8\1280,1024",,,"60,70,75"
HKR,"MODES\8\1600,1200",,,"48"
HKR,"MODES\16\640,480"
HKR,"MODES\16\800,600"
HKR,"MODES\16\1024,768"
HKR,"MODES\16\1280,1024"
HKR,"MODES\24\640,480"
HKR,"MODES\24\800,600"
HKR,"MODES\24\1024,768"

[ET6000.PosDup]
*PNP0912


; User visible strings
; ---------------------------------------------------------
[Strings]
MS="Microsoft"

Diamond="Diamond Multimedia Systems"
DFI="DFI"
Genoa="Genoa Systems"
Herc="Hercules Computer Technology"
Orchid="Orchid Technology"
STB="STB Systems"
Tseng="Tseng Labs"

*PNP0906.DeviceDesc="Tseng Labs ET4000"
*PNP0912.DeviceDesc="Tseng Labs ET4000/W32"
*PNP091A.DeviceDesc="Tseng Labs ET4000"

PCI\VEN_100C&DEV_3202.DeviceDesc="Tseng Labs ET4000/W32 PCI"
PCI\VEN_100C&DEV_3205.DeviceDesc="Tseng Labs ET4000/W32 PCI"
PCI\VEN_100C&DEV_3206.DeviceDesc="Tseng Labs ET4000/W32 PCI"
PCI\VEN_100C&DEV_3207.DeviceDesc="Tseng Labs ET4000/W32 PCI"
PCI\VEN_100C&DEV_3208.DeviceDesc="Tseng Labs ET6000 PCI"

Stealth32="Diamond Stealth 32 (Tseng)"
SpeedStar="Diamond SpeedStar (Tseng)"
SpeedStar24="Diamond SpeedStar 24 (Tseng)"

WG5000="DFI WG-5000 (Tseng)"

Phantom32="Genoa Phantom 32I (Tseng)"

Dynamite="Hercules Dynamite (Tseng)"
DynamitePro="Hercules Dynamite Pro (Tseng)"

ProDesII="Orchid ProDesigner II (Tseng)"

ErgoMCX="STB Ergo MCX (Tseng)"
LightSpeed="STB LightSpeed (Tseng)"
MVP-2X="STB MVP-2X (Tseng)"
MVP-4X="STB MVP-4X (Tseng)"

[SourceDisksNames]
222="DirectX Drivers Disk","",1

[SourceDisksFiles]
framebuf.drv=222
supervga.drv=222
tseng.drv=222
tseng.dll=222
tseng.vxd=222
et6000.drv=222
et6000.vxd=222
et6000.dll=222



